Enable

Show ip interface brief(sh ip int b)

Show ip route

Show running config (show run)

Show startup config (show start)

Config t (config)

Hostname name

Enable password pass

Enable secret pass

Line console 0

Password pass

Login

Exit

Service password-encryption

Banner motd “message to print”

copy running-config startup-config (cop r st)

copy startup-config flash

interface gigabitethernet 0/0

ip address 192.168.10.1 255.255.255.0

description LAN connection to S1

~~show ntp status~~

~~show clock detail~~

~~ntp server ipaddress~~

~~show ntp association~~